**Mini-Rhizotron Tube Installation**

Melissa Lucash 5/2002

Equipment Inventory

* Coring apparatus—can be dismantled into 2 pieces (DO NOT LOSE BOLTS)
* Corer
* 4 Apparatus anchors
* Corer Cap
* “Hammer”
* Soil probe
* Tubes
* (You will need duct tape, electrical tape, flagging)

Important things to remember:

* Coring depth is marked in black on corer
* Align tubes so that holes are @ 11-1-5-7
* Electrical tape up to holes
* Duct tape “cap”
* Flag tubes