{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":1,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["Copy the following to a .txt file and change the files paths between < > brackets and replace any \"#\" with your numbers.  Make no other changes! (might not read correctly)"]
["Input:"]
["Landcover file: <C:\\Folder\\land.txt>"]
["Treecover file: <C:\\Folder\\tree.txt>"]
["Impervious file: <C:\\Folder\\impervious.txt>"]
["RG Percentage of Watershed: <#>"]
[]
["Output Files:"]
["Base case param file: <C:\\Folder\\param_base.txt>"]
["RG Location file: <C:\\Folder\\RGloc.txt>"]
["New Tree cover file: <C:\\Folder\\RGtree.txt>"]
["New param file: <C:\\Folder\\param_RG.txt>"]
[]
["Initial Hydrological Parameters:"]
["# Tree LAI"]
["# Percent Evergreen Tree Cover"]
["# Percent Evergreen Shrub Cover"]
["# Shrub LAI"]
["# Herbaceous LAI"]
["# Connected Impervious to Stream"]
["# Scale parameter of soil transmissivity"]
["# Transmissivity at Saturation"]
["# Unsaturated zone time delay"]
["# Maximum root zone storage deficit"]
["# percent of watershed generating IEOF"]
["# Initial stream discharge"]
["# initial root zone deficit"]
["# main channel routing velocity"]
["# internal channel routing velocity"]
["# Wetting Front Suction"]
["# Wetted Moisture Content"]
["# Surface Hydraulic Conductivity"]
["# Impervious Depression Storage"]
["# Time constant of watershed"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}